<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<library>
<description>&lt;p&gt;&lt;b&gt;Commodore card edges&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="COMMODORE_PARALLEL_PORT_CARD_EDGE">
<description>&lt;p&gt;&lt;b&gt;Commodore 26-Contact (13 top + 13 bottom) Parallel Port Card-Edge.&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Contacts are 0.05" x 0.35" on a 0.1" pitch.&lt;/p&gt;
&lt;p&gt;Numbering alternates between top and bottom, with contact 1 at bottom. Contacts 1 and 2 are on same end of card-edge.&lt;/p&gt;
&lt;p&gt;There is a 0.05" gap between contacts 21/22 and 23/24.&lt;/p&gt;
&lt;p&gt;Card edge protrudes 0.55" from main circuit board.&lt;/p&gt;</description>
</package>
<package name="COMMODORE_IEEE-488_PORT_CARD_EDGE">
<description>&lt;p&gt;&lt;b&gt;Commodore 24-Contact (12 top + 12 bottom) IEEE-488 Port Card-Edge.&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Contacts are 0.09" x 0.35" on a 0.156" pitch.&lt;/p&gt;
&lt;p&gt;Contacts are numbered 1 to 12 on top and A to N on bottom (excludes G and I). Contacts 1 and A are on same end of card-edge.&lt;/p&gt;
&lt;p&gt;There is a 0.066" gap between contacts 2/B and 3/C and 9/K and10/L.&lt;/p&gt;
&lt;p&gt;Card edge protrudes 0.55" from main circuit board.&lt;/p&gt;</description>
</package>
<package name="COMMODORE_64_EXPANSION_PORT_CARD_EDGE">
<description>&lt;p&gt;&lt;b&gt;Commodore 64 44-Contact (22 top + 22 bottom) Expansion Port Card-Edge.&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Contacts are 0.05" x 0.35" on a 0.1" pitch.&lt;/p&gt;
&lt;p&gt;Contacts are numbered 1 to 22 on top and A to Z on bottom (excludes G, I, O, and Q). Contacts 1 and A are on same end of card-edge.&lt;/p&gt;
&lt;p&gt;Card edge protrudes 0.55" from main circuit board.&lt;/p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="COMMODORE_PARALLEL_PORT_CARD_EDGE">
<description>&lt;p&gt;&lt;b&gt;Commodore 26-Contact (13 top + 13 bottom) Parallel Port Card-Edge.&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Contacts are 0.05" x 0.35" on a 0.1" pitch.&lt;/p&gt;
&lt;p&gt;Numbering alternates between top and bottom, with contact 1 at bottom. Contacts 1 and 2 are on same end of card-edge.&lt;/p&gt;
&lt;p&gt;There is a 0.05" gap between contacts 21/22 and 23/24.&lt;/p&gt;
&lt;p&gt;Card edge protrudes 0.55" from main circuit board.&lt;/p&gt;</description>
<pin name="STROBE"/>
<pin name="GND@1" direction="pwr"/>
<pin name="PA0"/>
<pin name="GND@2" direction="pwr"/>
<pin name="PA1"/>
<pin name="GND@3" direction="pwr"/>
<pin name="PA2"/>
<pin name="GND@4" direction="pwr"/>
<pin name="PA3"/>
<pin name="GND@5" direction="pwr"/>
<pin name="PA4"/>
<pin name="GND@6" direction="pwr"/>
<pin name="PA5"/>
<pin name="GND@7" direction="pwr"/>
<pin name="PA6"/>
<pin name="GND@8" direction="pwr"/>
<pin name="PA7"/>
<pin name="GND@9" direction="pwr"/>
<pin name="N/C@1" direction="nc"/>
<pin name="GND@10" direction="pwr"/>
<pin name="BUSY"/>
<pin name="GND@11" direction="pwr"/>
<pin name="N/C@2" direction="nc"/>
<pin name="GND@12" direction="pwr"/>
<pin name="N/C@3" direction="nc"/>
<pin name="GND@13" direction="pwr"/>
</symbol>
<symbol name="COMMODORE_IEEE-488_PORT_CARD_EDGE">
<description>&lt;p&gt;&lt;b&gt;Commodore 24-Contact (12 top + 12 bottom) IEEE-488 Port Card-Edge.&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Contacts are 0.09" x 0.35" on a 0.156" pitch.&lt;/p&gt;
&lt;p&gt;Contacts are numbered 1 to 12 on top and A to N on bottom (excludes G and I). Contacts 1 and A are on same end of card-edge.&lt;/p&gt;
&lt;p&gt;There is a 0.066" gap between contacts 2/B and 3/C and 9/K and10/L.&lt;/p&gt;
&lt;p&gt;Card edge protrudes 0.55" from main circuit board.&lt;/p&gt;</description>
<pin name="DIO1"/>
<pin name="DIO2"/>
<pin name="DIO3"/>
<pin name="DIO4"/>
<pin name="EOI"/>
<pin name="DAV"/>
<pin name="NRFD"/>
<pin name="NDAC"/>
<pin name="IFC"/>
<pin name="SRQ"/>
<pin name="ATN"/>
<pin name="SHIELD" direction="pwr"/>
<pin name="DIO5"/>
<pin name="DIO6"/>
<pin name="DIO7"/>
<pin name="DIO8"/>
<pin name="REN"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
</symbol>
<symbol name="COMMODORE_64_EXPANSION_PORT_CARD_EDGE">
<description>&lt;p&gt;&lt;b&gt;Commodore 64 44-Contact (22 top + 22 bottom) Expansion Port Card-Edge.&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Contacts are 0.05" x 0.35" on a 0.1" pitch.&lt;/p&gt;
&lt;p&gt;Contacts are numbered 1 to 22 on top and A to Z on bottom (excludes G, I, O, and Q). Contacts 1 and A are on same end of card-edge.&lt;/p&gt;
&lt;p&gt;Card edge protrudes 0.55" from main circuit board.&lt;/p&gt;</description>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="!IRQ"/>
<pin name="R/!W"/>
<pin name="DOT_CLOCK"/>
<pin name="I/O1"/>
<pin name="!GAME"/>
<pin name="!EXROM"/>
<pin name="I/O2"/>
<pin name="!ROML"/>
<pin name="BA"/>
<pin name="!DMA"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="D5"/>
<pin name="D4"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="D1"/>
<pin name="D0"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="!ROMH"/>
<pin name="!RESET"/>
<pin name="!NMI"/>
<pin name="PHASE2"/>
<pin name="A15"/>
<pin name="A14"/>
<pin name="A13"/>
<pin name="A12"/>
<pin name="A11"/>
<pin name="A10"/>
<pin name="A9"/>
<pin name="A8"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="GND@4" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="COMMODORE_PARALLEL_PORT_CARD_EDGE" prefix="P" uservalue="yes">
<description>&lt;p&gt;&lt;b&gt;Commodore 26-Contact (13 top + 13 bottom) Parallel Port Card-Edge.&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Contacts are 0.05" x 0.35" on a 0.1" pitch.&lt;/p&gt;
&lt;p&gt;Numbering alternates between top and bottom, with contact 1 at bottom. Contacts 1 and 2 are on same end of card-edge.&lt;/p&gt;
&lt;p&gt;There is a 0.05" gap between contacts 21/22 and 23/24.&lt;/p&gt;
&lt;p&gt;Card edge protrudes 0.55" from main circuit board.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="COMMODORE_PARALLEL_PORT_CARD_EDGE"/>
</gates>
<devices>
<device name="" package="COMMODORE_PARALLEL_PORT_CARD_EDGE">
<connects>
<connect gate="G$1" pin="BUSY" pad="21"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@10" pad="20"/>
<connect gate="G$1" pin="GND@11" pad="22"/>
<connect gate="G$1" pin="GND@12" pad="24"/>
<connect gate="G$1" pin="GND@13" pad="26"/>
<connect gate="G$1" pin="GND@2" pad="4"/>
<connect gate="G$1" pin="GND@3" pad="6"/>
<connect gate="G$1" pin="GND@4" pad="8"/>
<connect gate="G$1" pin="GND@5" pad="10"/>
<connect gate="G$1" pin="GND@6" pad="12"/>
<connect gate="G$1" pin="GND@7" pad="14"/>
<connect gate="G$1" pin="GND@8" pad="16"/>
<connect gate="G$1" pin="GND@9" pad="18"/>
<connect gate="G$1" pin="N/C@1" pad="19"/>
<connect gate="G$1" pin="N/C@2" pad="23"/>
<connect gate="G$1" pin="N/C@3" pad="25"/>
<connect gate="G$1" pin="PA0" pad="3"/>
<connect gate="G$1" pin="PA1" pad="5"/>
<connect gate="G$1" pin="PA2" pad="7"/>
<connect gate="G$1" pin="PA3" pad="9"/>
<connect gate="G$1" pin="PA4" pad="11"/>
<connect gate="G$1" pin="PA5" pad="13"/>
<connect gate="G$1" pin="PA6" pad="15"/>
<connect gate="G$1" pin="PA7" pad="17"/>
<connect gate="G$1" pin="STROBE" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="COMMODORE_IEEE-488_PORT_CARD_EDGE" prefix="P">
<description>&lt;p&gt;&lt;b&gt;Commodore 24-Contact (12 top + 12 bottom) IEEE-488 Port Card-Edge.&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Contacts are 0.09" x 0.35" on a 0.156" pitch.&lt;/p&gt;
&lt;p&gt;Contacts are numbered 1 to 12 on top and A to N on bottom (excludes G and I). Contacts 1 and A are on same end of card-edge.&lt;/p&gt;
&lt;p&gt;There is a 0.066" gap between contacts 2/B and 3/C and 9/K and10/L.&lt;/p&gt;
&lt;p&gt;Card edge protrudes 0.55" from main circuit board.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="COMMODORE_IEEE-488_PORT_CARD_EDGE"/>
</gates>
<devices>
<device name="" package="COMMODORE_IEEE-488_PORT_CARD_EDGE">
<connects>
<connect gate="G$1" pin="ATN" pad="11"/>
<connect gate="G$1" pin="DAV" pad="6"/>
<connect gate="G$1" pin="DIO1" pad="1"/>
<connect gate="G$1" pin="DIO2" pad="2"/>
<connect gate="G$1" pin="DIO3" pad="3"/>
<connect gate="G$1" pin="DIO4" pad="4"/>
<connect gate="G$1" pin="DIO5" pad="A"/>
<connect gate="G$1" pin="DIO6" pad="B"/>
<connect gate="G$1" pin="DIO7" pad="C"/>
<connect gate="G$1" pin="DIO8" pad="D"/>
<connect gate="G$1" pin="EOI" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="F"/>
<connect gate="G$1" pin="GND@2" pad="H"/>
<connect gate="G$1" pin="GND@3" pad="J"/>
<connect gate="G$1" pin="GND@4" pad="K"/>
<connect gate="G$1" pin="GND@5" pad="L"/>
<connect gate="G$1" pin="GND@6" pad="M"/>
<connect gate="G$1" pin="GND@7" pad="N"/>
<connect gate="G$1" pin="IFC" pad="9"/>
<connect gate="G$1" pin="NDAC" pad="8"/>
<connect gate="G$1" pin="NRFD" pad="7"/>
<connect gate="G$1" pin="REN" pad="E"/>
<connect gate="G$1" pin="SHIELD" pad="12"/>
<connect gate="G$1" pin="SRQ" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="COMMODORE_64_EXPANSION_PORT_CARD_EDGE" prefix="P">
<description>&lt;p&gt;&lt;b&gt;Commodore 64 44-Contact (22 top + 22 bottom) Expansion Port Card-Edge.&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Contacts are 0.05" x 0.35" on a 0.1" pitch.&lt;/p&gt;
&lt;p&gt;Contacts are numbered 1 to 22 on top and A to Z on bottom (excludes G, I, O, and Q). Contacts 1 and A are on same end of card-edge.&lt;/p&gt;
&lt;p&gt;Card edge protrudes 0.55" from main circuit board.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="COMMODORE_64_EXPANSION_PORT_CARD_EDGE"/>
</gates>
<devices>
<device name="" package="COMMODORE_64_EXPANSION_PORT_CARD_EDGE">
<connects>
<connect gate="G$1" pin="!DMA" pad="13"/>
<connect gate="G$1" pin="!EXROM" pad="9"/>
<connect gate="G$1" pin="!GAME" pad="8"/>
<connect gate="G$1" pin="!IRQ" pad="4"/>
<connect gate="G$1" pin="!NMI" pad="D"/>
<connect gate="G$1" pin="!RESET" pad="C"/>
<connect gate="G$1" pin="!ROMH" pad="B"/>
<connect gate="G$1" pin="!ROML" pad="11"/>
<connect gate="G$1" pin="A0" pad="Y"/>
<connect gate="G$1" pin="A1" pad="X"/>
<connect gate="G$1" pin="A10" pad="M"/>
<connect gate="G$1" pin="A11" pad="L"/>
<connect gate="G$1" pin="A12" pad="K"/>
<connect gate="G$1" pin="A13" pad="J"/>
<connect gate="G$1" pin="A14" pad="H"/>
<connect gate="G$1" pin="A15" pad="F"/>
<connect gate="G$1" pin="A2" pad="W"/>
<connect gate="G$1" pin="A3" pad="V"/>
<connect gate="G$1" pin="A4" pad="U"/>
<connect gate="G$1" pin="A5" pad="T"/>
<connect gate="G$1" pin="A6" pad="S"/>
<connect gate="G$1" pin="A7" pad="R"/>
<connect gate="G$1" pin="A8" pad="P"/>
<connect gate="G$1" pin="A9" pad="N"/>
<connect gate="G$1" pin="BA" pad="12"/>
<connect gate="G$1" pin="D0" pad="21"/>
<connect gate="G$1" pin="D1" pad="20"/>
<connect gate="G$1" pin="D2" pad="19"/>
<connect gate="G$1" pin="D3" pad="18"/>
<connect gate="G$1" pin="D4" pad="17"/>
<connect gate="G$1" pin="D5" pad="16"/>
<connect gate="G$1" pin="D6" pad="15"/>
<connect gate="G$1" pin="D7" pad="14"/>
<connect gate="G$1" pin="DOT_CLOCK" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="22"/>
<connect gate="G$1" pin="GND@3" pad="A"/>
<connect gate="G$1" pin="GND@4" pad="Z"/>
<connect gate="G$1" pin="I/O1" pad="7"/>
<connect gate="G$1" pin="I/O2" pad="10"/>
<connect gate="G$1" pin="PHASE2" pad="E"/>
<connect gate="G$1" pin="R/!W" pad="5"/>
<connect gate="G$1" pin="VCC@1" pad="2"/>
<connect gate="G$1" pin="VCC@2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
