<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<library>
<packages>
<package name="FEMALE_44-PIN_CARD_EDGE_CONNECTOR">
<description>&lt;p&gt;&lt;b&gt;Female Connector for Commodore 64 44-Contact (22 top + 22 bottom) Expansion Port Card-Edge.&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Contacts are on a 0.1" (2.54 mm) pitch.&lt;/p&gt;
&lt;p&gt;Row pitch is 0.2" (5.08 mm).&lt;/p&gt;
&lt;p&gt;Contacts are numbered 1 to 22 on top and A to Z on bottom (excludes G, I, O, and Q). Contacts 1 and A are on same end of card-edge.&lt;/p&gt;
&lt;p&gt;Accepts board thickness of 0.062" (1.57 mm).&lt;/p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="FEMALE_44-PIN_CARD_EDGE_CONNECTOR">
<description>&lt;p&gt;&lt;b&gt;Female Connector for Commodore 64 44-Contact (22 top + 22 bottom) Expansion Port Card-Edge.&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Contacts are on a 0.1" (2.54 mm) pitch.&lt;/p&gt;
&lt;p&gt;Row pitch is 0.2" (5.08 mm).&lt;/p&gt;
&lt;p&gt;Contacts are numbered 1 to 22 on top and A to Z on bottom (excludes G, I, O, and Q). Contacts 1 and A are on same end of card-edge.&lt;/p&gt;
&lt;p&gt;Accepts board thickness of 0.062" (1.57 mm).&lt;/p&gt;</description>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="!IRQ"/>
<pin name="R/!W"/>
<pin name="DOT_CLOCK"/>
<pin name="I/O1"/>
<pin name="!GAME"/>
<pin name="!EXROM"/>
<pin name="I/O2"/>
<pin name="!ROML"/>
<pin name="BA"/>
<pin name="!DMA"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="D5"/>
<pin name="D4"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="D1"/>
<pin name="D0"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="!ROMH"/>
<pin name="!RESET"/>
<pin name="!NMI"/>
<pin name="PHASE2"/>
<pin name="A15"/>
<pin name="A14"/>
<pin name="A13"/>
<pin name="A12"/>
<pin name="A11"/>
<pin name="A10"/>
<pin name="A9"/>
<pin name="A8"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="GND@4" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="FEMALE_44-PIN_CARD_EDGE_CONNECTOR" prefix="P">
<description>&lt;p&gt;&lt;b&gt;Female Connector for Commodore 64 44-Contact (22 top + 22 bottom) Expansion Port Card-Edge.&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Contacts are on a 0.1" (2.54 mm) pitch.&lt;/p&gt;
&lt;p&gt;Row pitch is 0.2" (5.08 mm).&lt;/p&gt;
&lt;p&gt;Contacts are numbered 1 to 22 on top and A to Z on bottom (excludes G, I, O, and Q). Contacts 1 and A are on same end of card-edge.&lt;/p&gt;
&lt;p&gt;Accepts board thickness of 0.062" (1.57 mm).&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FEMALE_44-PIN_CARD_EDGE_CONNECTOR"/>
</gates>
<devices>
<device name="" package="FEMALE_44-PIN_CARD_EDGE_CONNECTOR">
<connects>
<connect gate="G$1" pin="!DMA" pad="13"/>
<connect gate="G$1" pin="!EXROM" pad="9"/>
<connect gate="G$1" pin="!GAME" pad="8"/>
<connect gate="G$1" pin="!IRQ" pad="4"/>
<connect gate="G$1" pin="!NMI" pad="D"/>
<connect gate="G$1" pin="!RESET" pad="C"/>
<connect gate="G$1" pin="!ROMH" pad="B"/>
<connect gate="G$1" pin="!ROML" pad="11"/>
<connect gate="G$1" pin="A0" pad="Y"/>
<connect gate="G$1" pin="A1" pad="X"/>
<connect gate="G$1" pin="A10" pad="M"/>
<connect gate="G$1" pin="A11" pad="L"/>
<connect gate="G$1" pin="A12" pad="K"/>
<connect gate="G$1" pin="A13" pad="J"/>
<connect gate="G$1" pin="A14" pad="H"/>
<connect gate="G$1" pin="A15" pad="F"/>
<connect gate="G$1" pin="A2" pad="W"/>
<connect gate="G$1" pin="A3" pad="V"/>
<connect gate="G$1" pin="A4" pad="U"/>
<connect gate="G$1" pin="A5" pad="T"/>
<connect gate="G$1" pin="A6" pad="S"/>
<connect gate="G$1" pin="A7" pad="R"/>
<connect gate="G$1" pin="A8" pad="P"/>
<connect gate="G$1" pin="A9" pad="N"/>
<connect gate="G$1" pin="BA" pad="12"/>
<connect gate="G$1" pin="D0" pad="21"/>
<connect gate="G$1" pin="D1" pad="20"/>
<connect gate="G$1" pin="D2" pad="19"/>
<connect gate="G$1" pin="D3" pad="18"/>
<connect gate="G$1" pin="D4" pad="17"/>
<connect gate="G$1" pin="D5" pad="16"/>
<connect gate="G$1" pin="D6" pad="15"/>
<connect gate="G$1" pin="D7" pad="14"/>
<connect gate="G$1" pin="DOT_CLOCK" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="22"/>
<connect gate="G$1" pin="GND@3" pad="A"/>
<connect gate="G$1" pin="GND@4" pad="Z"/>
<connect gate="G$1" pin="I/O1" pad="7"/>
<connect gate="G$1" pin="I/O2" pad="10"/>
<connect gate="G$1" pin="PHASE2" pad="E"/>
<connect gate="G$1" pin="R/!W" pad="5"/>
<connect gate="G$1" pin="VCC@1" pad="2"/>
<connect gate="G$1" pin="VCC@2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
